Casio CTK-750

Chip: TC5316200CP (5V 16bit)

Print:
~~~~~~~~~~~~~~~
 TOSHIBA
 TC5316200CP
 C081
 JAPAN 9348EAI
~~~~~~~~~~~~~~~

Contains a lot of excellent samples in signed linear 8bit and signed intel linear 16bit formats.
Contains strings "TESTOFDATA19931201  SAKITABLE---".

Endinanness in your programming tools may be reversed.
To ensure that what you burn matches the necessary endianness, you'll have to dump
the old rom from your device through your tools and compare byte sequence with this one.
Swap bytes if necessary, and then burn that data.


Edward d-tech
www.dtech.lv
