Yamaha PSR730

Update kit label:
XS988603   IC EP 16M M27C160-100FI V6.03 PSR730

PSR730 V6.03 "XS988603" - combines to 32bit

Also added properly combined binary for reasearch and fun.

Mark at the end of the rom is "1001997JUN12185229" which likely translates to: version 1.00 1997/JUN/12 18:52:29

I also included extracts of all demo songs for your sequencing delight. With slight modifications to instrument mappings (or not) these
can be nicely used to test drive all kinds of GM-ish midi synth modules (especially waveblaster-type boards and other odd things).
For some reason I personally do realy enjoy running "wrong" demos on all the "wrong" synths that normally should have never
happened - like Roland XP-10 demos on PSR-230 and such.


Chips: M27C160

Print:
~~~~~~~~~~~~~~~~
 (c)1997 YAMAHA
     XS98810
~~~~~~~~~~~~~~~~

~~~~~~~~~~~~~~~~
 (c)1997 YAMAHA
     XS98910
~~~~~~~~~~~~~~~~


Endinanness in your programming tools may be reversed.
To ensure that what you burn matches the necessary endianness, you'll have to dump
the old rom from your device through your tools and compare byte sequence with this one.
Swap bytes if necessary, and then burn that data.


Edward d-tech
www.dtech.lv
