Yamaha PSR-79

Chip: 16bit 3.3V MX23L8100PC-10

Print:
~~~~~~~~~~~~~~~~~~
 MX J983351
    c 1998 YAMAHA
    XU66710
    1A1226Y2
~~~~~~~~~~~~~~~~~~

Update kit (spares) part label:
"XU667100   IC 8M MX23L8100PC-10"

Also included lossless conversion of waves for your sampling delight.

Endinanness in your programming tools may be reversed.
To ensure that what you burn matches the necessary endianness, you'll have to dump
the old rom from your device through your tools and compare byte sequence with this one.
Swap bytes if necessary, and then burn that data.


Edward d-tech
www.dtech.lv
